Processing module STM 3.0.20.upgrade file to be used along with Racelogic Upgrader v1.33b6 or later via RLCAB250.

firmware.upgrade file to be copied across to an SD card, inserted into the VIPSRPM-V2 via the SD card slot, and wait for flashing green on the log LED to signal a successful upgrade.